! Conductivity and diel-constant for differend grounds
! Format: <Name> = <condictivity>,<dielectric_constant>

Salt water              = 5,      81
Fresh water             = 0.001,  80
Past.,Rich (V-good)     = 0.0303, 20
Past.,low-hills (Good)  = 0.001,  14
Flat, marshy            = 0.0075, 12
Med-hills/forest        = 0.006,  13
Clay/forest (Average)   = 0.005,  13
Mountain area (Poor)    = 0.002,  13
Flat,sandy,dry          = 0.002,  10
Cities,indust.(V-poor)  = 0.001,  5
Big cities (Ext-poor)   = 0.001,  3
<user specified>        =      ,
